
Normal Approach and Landing (MPH)
Verify pattern altitude and weather no later than 10 nm from airport. 
45 degree entry
Begin slowing to 100 MPH and plan decent to enter the pattern. 
Downwind 
Abeam touchdown point complete before landing checklist, add carb heat, reduce power to 1500 rpm, set flaps 10, descend at 90 MPH.
Base
Final 
Turn base 45 degree angle from touchdown point.
Select flaps 20 and slow to 80 MPH.
Select flaps 30 and slow to 75 MPH.
Aiming Point 
Touchdown Point 
100 MPH Approx 2100 RPM
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